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DISASSEMBLY AND REPAIR
Product: A22
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	Replaceable parts
	Tools needed

	Glides
	Adjustable pillars, rubber mallet

	Seat pad
	-


Instructions for replacement
Glides	Remove the glide with adjustable pillars. Insert the new glide and tap with a rubber mallet.
Seat pad	Separate the Velcro underneath the seat by hand. Attach the new seat pad.



Disassembly for recycling
Remove the glide with adjustable pillars. Remove the seatpad.
image1.jpeg




image2.png




