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DISASSEMBLY AND REPAIR
Product: ADD
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	Replaceable parts
	Tools needed

	Backrest
	Screwdriver

	Seat
	Screwdriver







Instructions for replacement
Seat	Loosen all screws with a screwdriver and remove the backrest. Attach the new seat and reattach the backrest.
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Backrest	To be able to replace the backrest, you need to order a new, assembled backrest. Loosen the backrest screws with a screwdriver and replace the existing backrest with the new one. Recycle the old one by separating the parts, using a rubber mallet to strike the backrest. 



Disassembly for recycling
Loosen all screws with a screwdriver to remove the seat and backrest. Use a rubber mallet to separate the backrest from the bracket. To remove the plastic glides, use a Ø5mm drill and drill out the pop rivets.
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