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DISASSEMBLY AND REPAIR
Product: ATTACH 
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	Replaceable parts
	Tools needed

	End caps
	Knife

	Glides
	-

	Legs
	Allen key

	Profiles
	Screwdriver, assembly board (multiple tabletops)

	Tabletop
	Screwdriver, assembly board (multiple tabletops)





Instructions for replacement
End cap	Use a knife or another thin tool to remove it. Push the new one in place. 
Glides 	Remove the plastic part with your hand and klick on the new glide
Leg	Loosen the screws if the leg is permanently fixed. Pull the leg of the beam. Click on the new leg, make sure it’s in correct position.[image: ]

[image: ]





[image: ]





Profile	Follow the Attach disassembly instruction to remove the profile. Then follow the Attach assembly instructions to assemble the new table. For tables with more than one tabletop, always use the assembly board.
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Tabletop	Follow the Attach disassembly instruction to remove the tabletop. Then follow the Attach assembly instructions to assemble the new table. For tables with more than one tabletop, always use the assembly board.
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Disassembly for recycling
Follow the separate disassembly instruction.
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Loosen screws if legs
are permanently fixed.
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