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DISASSEMBLY AND REPAIR
Product: CAMPUS 
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	Replaceable parts
	Tools needed

	Armrests
	Screwdriver

	Glides
	Adjustable pliers, rubber mallet

	Seat
	Screwdriver


Instructions for replacement
Armrest	Use a screwdriver to loosen the screws and remove the armrest. Put the new one in place and tighten the screws. Make sure the countersunk hole is pointing outwards to fit the screw.
Glides	Pull off the glide with adjustable pliers. Insert the new glide, position it correct and strike it with a rubber mallet.
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Seat (fabric)	Place the chair upside down on a table and use a screwdriver to remove the screws, 3 in the front and 2 in the back. Remove the old seat and replace it with the new one. Make sure the new seat has all bumpers in place. Start by tighten the screw placed in the middle front hole, to make sure that the frame is in position. Continue with the remaining screws.
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Seat (wood)	Place the chair upside down on a table and use a screwdriver to remove the screws, 3 in the front and 2 in the back. Remove the old seat and replace it with the new one. Place the plastic distances, one for each hole. Gently place the base on top without dislocating them. Use a screwdriver to fasten the screws, 5 pcs of MF6S 5x22.
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Disassembly for recycling
Place the chair upside down on a table and use a screwdriver to remove the seat and stacking bumpers. Remove the armrest in the same way. To remove the backrest, saw the back in half down the middle and twist the parts to detach them from the frame. Pull off the glide with adjustable pliers. 
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