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DISASSEMBLY AND REPAIR
Product: CAMPUS AIR SLED BASE




[image: ]


	Replaceable parts
	Tools needed

	Glides
	Screwdriver

	Seat
	Screwdriver




Instructions for replacement
Glides	Place the chair upside down on a table and use a screwdriver to remove the old glides. Put the new ones in place and tighten the screws.
Seat	Place the chair upside down on a table and use a screwdriver to remove the screws. Remove the old seat and replace it with the new one. Start by tighten the screw placed in the middle front hole, to make sure that the frame is in position. Continue with the remaining screws.


Disassembly for recycling
Place the chair upside down on a table and use a screwdriver to remove the seat. To remove the backrest, saw the back in half down the middle and twist the parts to detach them from the frame. Pull off the glides with adjustable pliers. To remove the armrests, use a screwdriver to loosen the screws and strike the armrest with a rubber mallet to separate it from the frame. 
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